Labbook

|  |  |
| --- | --- |
| Date / Time | Event |
| 27.07.2019, 16:05 UTC | Raining, start SMPS and compare the CPCs, switching valve is on. |
| 29.07.2019  6:30 UTC | Turn off the inlet pumps |
| 29.07.2019 13:39 | Fill butanol into 3025, intercompare the two cpcs, over night with putting on the inlet pumps as well |
| 30.07.2019  11:04 | Turn off inlet pumps |
| 30.07.2019  13:31 | Remove 3025 for intercomparison with PSM CPC |